{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":55,"n_cols":8,"rows_kept":55,"cut":false,"hidden":false,"merged":[[52,1,52,7],[53,1,53,7],[54,1,54,7],[55,1,63,7],[48,3,48,6],[44,1,44,2],[44,3,44,6],[45,1,45,2],[45,3,45,6],[50,1,50,2],[50,3,50,6],[36,3,36,6],[49,1,49,2],[49,3,49,6],[46,1,46,2],[46,3,46,6],[47,1,47,2],[47,3,47,6],[48,1,48,2],[39,1,39,2],[39,3,39,6],[28,3,28,6],[29,3,29,6],[30,3,30,6],[38,1,38,2],[38,3,38,6],[28,1,28,2],[29,1,29,2],[35,1,35,2],[35,3,35,6],[36,1,36,2],[43,1,43,7],[23,1,23,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[24,1,24,2],[24,3,24,6],[37,1,37,2],[37,3,37,6],[30,1,30,2],[3,1,3,7],[18,5,18,6],[22,1,22,2],[22,3,22,6],[15,3,15,4],[21,1,21,7],[15,1,15,2],[11,1,11,7],[12,1,12,7],[42,1,42,7],[23,3,23,6],[25,3,25,6],[26,3,26,6],[27,3,27,6],[5,3,5,5],[10,1,10,2],[14,1,14,2],[14,3,14,4],[14,5,14,6],[1,1,1,7],[2,1,2,7],[4,1,4,2],[5,1,5,2],[8,1,8,2],[32,1,32,7],[18,3,18,4],[16,1,16,2],[17,1,17,2],[18,1,18,2],[33,1,33,7],[34,1,34,7],[41,1,41,7],[6,1,6,2],[6,3,6,5],[4,6,6,7],[8,3,10,7],[9,1,9,2],[4,3,4,5],[17,5,17,6],[13,1,13,7],[19,1,19,7],[20,1,20,7],[15,5,15,6],[16,3,16,4],[16,5,16,6],[17,3,17,4]],"flags":["formulas_cached_only"]}
[]
[null,"Fragebogen zur Auslegung eines Elektro-Erhitzers"]
[null,"Questenair for design of a electric heater"]
[null,"Вопросник для проектирования электрического нагревателя"]
[null,"Art des Erhitzer",null,"Vorwärmen / preheating / предв. подогрев"]
[null,"Kind of heater",null,"Verdampfen / evaporating / испарение"]
[null,"Вид нагревателя"]
[]
[null,"Medium "]
[null,"Medium "]
[null,"Среда"]
[null,"Physikalische Kenndaten des Mediums bei Ein- und Austrittstemperatur und Betriebsdruck "]
[null,"Physical properties of medium @ inlet and outlet temperature and operation pressure"]
[null,"Физические свойства среды и входная и выходная температура и рабочее давление"]
[null,"Benennung / Desciption / Описание",null,"Eintritt / Inlet / Вход",null,"Austritt / outlet / Выход"]
[null,"Dichte\nDensity\nПлотность",{"$nulls":5},"kg/m³"]
[null,"Wärmekapazität \nheat capacity\nТеплоемкость",{"$nulls":5},"kJ/kg K"]
[null,"Wärmeleitfähigkeit\nheat conductivity\nТеплопроводность",{"$nulls":5},"W/mK"]
[null,"Dyn Viskosität\ndyn. Viscosoty\nДинамическая вязкость",{"$nulls":5},"Pas"]
[null,"Betriebsbedingungen (falls vorgegeben)"]
[null,"Operation Conditions (if given)"]
[null,"Рабочие параметры (если заданы)"]
[null,"Benennung / Desciption / Описание"]
[null,"Eintrittstemperatur\nintlet temperature\nТемпература на входе",{"$nulls":5},"°C"]
[null,"Austrittstemperatur\noutlet temperature\nТемпература на выходе",{"$nulls":5},"°C"]
[null,"Massenstrom\nmass flow\nМассовый расход",{"$nulls":5},"kg/s"]
[null,"Installierte Leistung\ninstalled power\nУстановленная мощность",{"$nulls":5},"kW"]
[null,"Betriebsdruck\noperation pressure\nРабочее давление",{"$nulls":5},"bar g"]
[null,"zul. Druckverlust\nallowable pressure drop\nДопустимый перепад давления",{"$nulls":5},"bar"]
[null,"Grenztemp. Medium \nlimit tem. Medium\nТемпературный предел среды",{"$nulls":5},"°C"]
[null,"max. zul. Oberflächenbel.\nMax. all. Surface load\nМаксимально допустимая нагрузка на поверхность",{"$nulls":5},"W/cm²"]
[]
[null,"Auslegungsbedinung (falls vorgegeben)"]
[null,"Design Conditions (if given)"]
[null,"Расчетные условия (если заданы)"]
[null,"Benennung / Desciption / Описание"]
[null,"Auslegunsdruck\nDesign pressure\nРасчетное давление",{"$nulls":5},"bar g"]
[null,"Auslegungstemperatur\nDesign temperature\nРасчетная температура",{"$nulls":5},"°C"]
[null,"Korrosionszuschlag \ncorrosion allowance\nДопуск на коррозию",{"$nulls":5},"mm"]
[null,"Auslegungsstandard\nDesign standard \nСтандарт проектирования",null,"DGRL (PED) / ASMEVIII DIV.1  code stamped\nChina License / GOST"]
[]
[null,"Elektrische Daten "]
[null,"Electircal Data"]
[null,"Данные по электрике"]
[null,"Benennung / Desciption / Описание"]
[null,"Anschlussspannung\nInput supply voltage\nНапряжение на входе",{"$nulls":5},"V"]
[null,"Spannungstoleranz\nVoltage tolerance\nДопустимое отклонение напряжения",{"$nulls":5},"%"]
[null,"Leistungstoleranz\nPower tolerance\nДопуск по мощности",{"$nulls":5},"%"]
[null,"Wetterschutzart\nIP Protection\nСтепень защиты IP",null,"IP ??"]
[null,"Explosionsschutz \nexplosion protection\nВзрывозащита",null,"Zone / Gasgruppe / Temperaturklasse\nZone / gasgroup / temperature class\nЗона / газовая группа / температурный класс"]
[null,"Schaltanlage\ncontrol unit\nБлок управления",null,"Stufenschaltung / Stufenlos\ntap change operation (step control) / stepless cont.\nПошаговое управление / бесступенчатый контроль"]
[]
[null,"Bemerkung"]
[null,"Remark"]
[null,"Примечание"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}